##
##  flowscan-cuflow.cf -- flowscan(1) CUFlow reporter configuration
##

#   the Round-Robin-Database (RRD) storage location
OutputDir @l_prefix@/var/flowscan/cuflow/rrd

#   generate top N and over-time-average top N reports
Scoreboard     10 @l_prefix@/var/flowscan/cuflow/web               @l_prefix@/var/flowscan/cuflow/web/topten.html
AggregateScore 10 @l_prefix@/var/flowscan/cuflow/web/aggregate.txt @l_prefix@/var/flowscan/cuflow/web/overall.html

#   multicast tracking support
Multicast

#   the NetFlow exporters
Router 192.168.0.1 router1.example.com
Router 192.168.0.2 router2.example.com

#   subnets (to determine whether a packet is inbound our outbound)
Subnet 192.168.0.0/24

#   track by networks
Network 192.168.0.0/24                example.com
Network 192.168.0.1/32,192.168.0.2/32 host.example.com

#   track by services
Service 20-21/tcp                   ftp
Service 22/tcp                      ssh
Service 23/tcp                      telnet
Service 25/tcp                      smtp
Service 53/udp,53/tcp               dns
Service 69/udp                      tftp
Service 80/tcp                      http
Service 110/tcp                     pop3
Service 111/udp,111/tcp             sunrpc
Service 113/tcp                     ident
Service 119/tcp                     nntp
Service 123/udp,123/tcp             ntp
Service 142-143/tcp                 imap
Service 161-162/udp                 snmp
Service 389/tcp                     ldap
Service 443/tcp                     https
Service 514/udp                     syslog      
Service 540/tcp                     uucp      
Service 563/tcp                     nntps
Service 636/tcp                     ldaps
Service 873/tcp                     rsync
Service 989-990/tcp                 ftps
Service 993/tcp                     imaps
Service 995/tcp                     pop3s
Service 1645-1646/udp,1812-1813/udp radius
Service 194/tcp,6665-6669/tcp       irc

#   track by protocols
Protocol 1   icmp
Protocol 6   tcp
Protocol 17  udp
Protocol 112 vrrp

#   track by ToS
TOS 0     normal
TOS 1-255 other

