<file name="config">
##
##  config -- UUCP main configuration
##

sysfile                @l_prefix@/etc/uucp/config.sys
portfile               @l_prefix@/etc/uucp/config.port
dialfile               @l_prefix@/etc/uucp/config.dial
dialcodefile           @l_prefix@/etc/uucp/config.dialcode
callfile               @l_prefix@/etc/uucp/config.passwd.out
passwdfile             @l_prefix@/etc/uucp/config.passwd.in

logfile                @l_prefix@/var/uucp/log/uucp.log
statfile               @l_prefix@/var/uucp/log/uucp.stat
debugfile              @l_prefix@/var/uucp/log/uucp.debug   
pubdir                 @l_prefix@/var/uucp/public
spool                  @l_prefix@/var/uucp/spool
lockdir                @l_prefix@/var/uucp/lock

nodename               openpkg

max-uuxqts             5                
timetable              Day Wk0801-1959

unknown commands
unknown pubdir         @l_prefix@/var/uucp/public
unknown remote-send    ~ !~/incoming
unknown remote-receive ~/incoming

</file>
<file name="config.dial">
##
##  config.dial -- UUCP dialer configuration
##

#   modem with Hayes command set
dialer       hayes
chat         "" ATZ\r\d\c OK ATDT\T CONNECT
chat-timeout 60
chat-fail    BUSY
chat-fail    NO\sCARRIER
complete     \d\d+++\d\dATH\r\c
abort        \d\d+++\d\dATH\r\c

#   direct connections
dialer       direct
chat         "" ""

#   modem direct
dialer       modem_direct
chat         "" \r\dAT\r\c
complete     \rATH\r\c
abort        \rATH\r\c

#   modem for use with UUCP
dialer       modem_uucp
chat         "" \d\d\r\dAT\r\c OK ATDT\D\r\c\d CONNECT ""
chat-fail    BUSY
chat-fail    NO\sCARRIER
complete     \d\d+++\d\dATH\r\cATZ
abort        \d\d+++\d\dATH\r\cATZ

</file>
<file name="config.dialcode">
##
##  dialcode -- TaylorUUCP dialcode file
##

#   The dialcode file is used if \T is used in the dialer chat script
#   and the telephone number begins with alphabetic characters.  The
#   alphabetic characters are looked up and translated in dialcode.
#   For example, if the phone number (from the sys file) is MA7389449,
#   then the string sent to the modem will be 6177389449.

MA 617
CA 415

</file>
<file name="config.passwd.in">
##
##  config.passwd.in -- UUCP password file for incoming calls
##

#   This file is used when uucico is invoked with the -l or -e argument.
#   uucico will then prompt for a login name and password.  The login
#   name is looked up in this file to check the password (the system
#   password file, /etc/passwd, is not checked).  This permits uucico to
#   completely take over a port, allowing UUCP access to remote systems
#   but not permitting remote users to actually log in to the system.
#   The format is just login-name password.

</file>
<file name="config.passwd.out">
##
##  config.passwd.out -- UUCP password file for outgoing calls
##

#   This file is used when the ``call-login'' or ``call-password''
#   commands are used in the sys file with a "*" argument (e.g.,
#   ``call-login *'').  The system name is looked up in this file, and
#   the login name and password are used.
#   The point of this is that the sys file may then be publically
#   readable, while still concealing the login names and passwords used
#   to connect to the remote system.
#   The format is just system-name login-name password.

foo Ufoo foopw

</file>
<file name="config.port">
##
##  config.port -- UUCP port configuration
##

port     tcp-direct
type     tcp

port     ssl-direct
type     pipe
command  @l_prefix@/sbin/stunnel @l_prefix@/etc/uucp/config.ssl

port     modem-direct
type     modem
device   /dev/cuaa0
speed    115200
dialer   modem_direct

port     modem-uucp
type     modem
device   /dev/cuaa0
speed    115200
dialer   modem_uucp

</file>
<file name="config.sys">
##
##  config.sys -- UUCP remote system configuration
##

#   defaults for all systems listed in this file
call-login         *
call-password      *
local-send         /
local-receive      /
time               any
commands           uucp rmail rnews rcsmtp
command-path       @l_prefix@/bin @l_prefix@/sbin /bin /usr/bin /usr/local/bin
forward            any
chat-timeout       60
chat               ogin: \L sword: \P
protocol           g
protocol-parameter g timeout 60
protocol-parameter g retries 10

#  sample modem direct connection
system             modem
port               modem-direct

#  sample peer connection
system             foo
alias              foobox
myname             openpkg
time               Any
port               tcp-direct
address            uucp.example.com
chat-timeout       120
protocol           t
protocol-parameter t timeout 60
protocol-parameter t retries 10

</file>
<file name="config.ssl">
##
##  config.ssl -- UUCP stunnel(1) configuration for UUCP-over-SSL
##

client      = yes
foreground  = yes
output      = /dev/null
connect     = uucp.example.com:4031

</file>
